**cid:image001.jpg@01C8D0A5.F08999B0 BARBECUE PITS BY KLOSE-DELIVERY WORLD WIDE cid:image002.gif@01C8D0A5.F08999B0   
BBQ Pits by Klose 1355 JUDIWAY STREET #B Houston, Texas 77018-6005  
Phone: 713-686-8720 Factory Floor Fax: 713-686-8793 Toll Free: 1-800-487-7487  
Website:** [**WWW.BBQPITS.COM**](http://www.bbqpits.com/) **Email:** [**david@bbqpits.com**](mailto:david@bbqpits.com)

****

**An Amazing New Design Open Grill with all Stainless Steel interior Liners, Firebox, & Meat Racks.**

**Front SS Removable Drip Shield, Catch Pans, & SS Angle Hot Coal Guard/**

**Firebox Rack with Removable SS Solid Sides. Built to Last A Lifetime of Use.**

**Boat Winches with SS Cable to Elevate the Rear of the SS Meat Racks for Food Product Displays.**

****

**cid:image001.jpg@01C8D0A5.F08999B0 BARBECUE PITS BY KLOSE-DELIVERY WORLD WIDE cid:image002.gif@01C8D0A5.F08999B0   
BBQ Pits by Klose 1355 JUDIWAY STREET #B Houston, Texas 77018-6005  
Phone: 713-686-8720 Factory Floor Fax: 713-686-8793 Toll Free: 1-800-487-7487  
Website:** [**WWW.BBQPITS.COM**](http://www.bbqpits.com/) **Email:** [**david@bbqpits.com**](mailto:david@bbqpits.com)

****

****

**An Amazing New Design Open Grill with all Stainless Steel interior Liners, Firebox, & Meat Racks.**

**Front SS Removable Drip Shield, Catch Pans, & SS Angle Hot Coal Guard 17,975.00**

**Firebox Rack with Removable SS Solid Sides. Built to Last A Lifetime of Use.**

**Boat Winches with SS Cable to Elevate the Rear of the SS Meat Racks for Food Product Displays.**

**HOT COAL BED RACK ON BOTTOM OF FIREBOX MADE FROM 1-1/2” THICK STEEL**

**36” deep by 8 foot long open grill with 14” tall sides, on 8” locking swivel caster legs**

**outside A36, grade new steel plate & painted food grade BBQ Black**

**Legs made from 3” x ¼ wall steel pipe & painted food grade BBQ Black**

**Firebox Solid Stainless Steel, & double wall SS lined 2” thick with rock wool Insulation,**

**Now Comes With 3/8” Ss Plate 16” Over Firebox To Protect Ansel Supression Systems.**

**304 stainless steel components:**

**Full Interior Liner of ¼” Thick Stainless Steel riveted with SS Rivets**


**Removable 4” deep V-grooved grease drain attached to front of grill w/ ss drip catch’s**

**Meat racks made from 1” ss angle framing ½” ss solid round bars,**

**allowing to be tilted up 35 degrees on ss cable for display**

**Fire rack made from solid ss plate & angles, with removable solid ss plate sides.**

**Other components: Two Standard 2,000# boat winches w/ SS Cables**

****